# Kinematics and Dynamics of Fixed Wing UAVs

Vladimir, Dobrokhodov

Naval Postgraduate School, Mechanical and Aerospace Engineering department

Monterey, CA

United States

## Abstract

The chapter provides a review of fundamental knowledge required for accurate mathematical modelling of flight of a fixed wing UAV. The key building blocks required for accurate modelling include the kinematics and dynamics of motion, and the transformation of forces and moments acting on the airplane. The detailed discussion of the “Kinematics-Dynamics-Actions” triad in application to a generic fixed wing UAV is the main objective of this chapter. Therefore, the presentation starts with an introduction to the coordinate frames, their transformations and differential rotations. Kinematics of the coordinate frames is what connects states of a fixed wing UAV and transforms forces and moments acting in different coordinate frames. Understanding of reference frames and their dynamics is essential for the guidance, navigation and control systems design. Next, the chapter provides a detailed derivation of the equations of motion using the Newtonian approach. Assuming that a fixed wing UAV can be represented as a rigid body moving in an inertial space, allows for the derivation of the linear and angular momentum equations. Starting in an inertial frame, it is shown how the final form of translational and rotational equations of motion become written in a body fixed coordinate frame. The development of both the kinematic and dynamic equations is carried out first in a general vector form; then, using simplifying assumptions applicable to a generic fixed wing symmetric UAV, the vector equations are expanded into a scalar form to better represent the details of remaining terms. Finally, the chapter presents the principles of defining the forces and moments acting on a generic fixed wing airplane. Since the forces and moments found on an airplane act in a number of coordinate frames including inertial, body fixed and wind frames, the chapter utilizes the concepts and tools built in the kinematics section to transform the forces and moments into the body fixed frame. Such transformations complete the presentation of the “Kinematics-Dynamics-Actions” triad.

## Introduction

The chapter objective is to provide an overview of the necessary theoretical material to enable a reliable mathematical modelling of the free and controlled motion of a generic fixed wing UAV. Besides the equations of motion describing the kinematics and dynamics of a rigid body motion, the tools and methods developed in this chapter contribute significantly into the UAV flight dynamics, system identification, control, guidance and navigation. Although the subject is not new and is well presented in existing literature, the rapid advancements of the last decade in research and development of fixed wing UAV technologies open new applications that require a revision of the existing assumptions. New materials, novel structural designs, new aerodynamic configurations, advanced onboard instrumentation including miniature sensors, actuators, and tremendous onboard processing power enable much wider operational envelop of fixed wing UAVs and significantly higher utility of their payloads. Depending on the UAV configuration and its intended operational use, the standard 12 equations of motion might not suffice for the task at hand and require deeper consideration of the UAV components interaction.

The chapter starts with some preliminaries required to describe kinematics of a rigid body motion in three dimensional (3D) space. Thus, the kinematics of 3D rotation is introduced first. The most commonly used coordinate frames that are utilized in the description of UAV states are presented next. Applying the kinematics of rotating frames to a set of specific coordinate frames builds the basis for a convenient description of the forces and moments acting on a fixed wing airplane. Understanding of reference frames and their dynamics is essential for the eventual development of the guidance, navigation and control systems architecture. Next, the chapter provides a detailed derivation of the equations of motion using the classical Newtonian approach. Assuming that a fixed wing UAV can be represented as a rigid body moving in an inertial space allows for the derivation of the linear and angular momentum equations. Starting in an inertial frame, it is shown how the final form of translational and rotational equations of motion become written in a body fixed coordinate frame. The development of both the kinematic and dynamic equations is carried out first in a general vector form, and then, using simplifying assumptions applicable to a generic fixed wing symmetric UAV, the vector equations are expanded into a scalar form to better represent the details of the remaining terms. A conceptual review of the approaches used to model the aerodynamic, propulsion, gravity and turbulent atmosphere forces and moments completes the formal definition of the equations of motion. Since the forces and moments found on an airplane act in a number of coordinate frames including inertial, body fixed and wind frames, the chapter utilizes the concepts and tools built in the kinematics description to transform the forces and moments into the body fixed frame. Thus, the complete derivation of linear and angular momentum equations, along with the accurate definition of the forces and moments acting on a rigid body, result in the generalized set of 6 Degree of Freedom (6DOF) equations of motion.

## Reference Frames and Coordinate Transformations

In order to accurately describe a body motion, it is required to define (i) the forces and moments acting on the body and thus resulting in the body motion, and (ii) the coordinate system that can be used as a reference for the motion states definition. It is important to note that there are two types of forces acting on a body in free motion. First, the inertial forces and moments that depend on the velocities and accelerations relative to an inertial reference frame; the classical Newtonian dynamics equations hold only in the inertial frame. The second group consists of the aerodynamic forces and moments resulting from interaction of the body with the surrounding airflow and therefore relative to the air. Since the airflow might not be stationary and in turn can be arbitrarily moving with respect to the body, it is therefore convenient to describe the resulting aerodynamics in the coordinate frames connected to the body and to the surrounding air. The resulting motion can be conveniently described in terms of the position, velocity, acceleration and attitude coordinates which comprise the states of the moving body. Some of these states, in turn, need to be defined with respect to a reference frame which choice is defined by the specifics of the UAV application. Thus, the information carried by various reference frames is what facilitates the complete and convenient definition of the free body motion.

Therefore, the section starts with a generalized definition of a coordinate frame and the description of the coordinate frame rotation. The reference frames required to represent the aerodynamic forces and moments and facilitating the solution of the navigation states are introduced next. Communication of the states information occurring during the coordinate frame transformation is presented for the major coordinate frames. The section ends with a set of kinematic equations required to represent the transition of linear and angular accelerations.

### Kinematics of moving frames

The objective of this subsection is to define a coordinate frame transformation and the associated mathematical formalism. Namely, the direct cosine matrix is introduced and its key properties are presented. The rotational matrix formalism is then followed by a differential rotation that defines the rate of change of the rotation matrix. A fundamental property of the simple summation of angular rates is introduced next. The section ends with a detailed presentation of the coordinate frames used to describe the 6DOF motion of a rigid body. The formal results of this initial development are heavily utilized throughout the entire chapter.

An arbitrary motion of a rigid body can be described by a transformation that consists of (Goldstein 1980) translational and rotational components. First, address the pure rotation of a rigid body. Consider a vector  defined in two orthogonal coordinate frames rotated with respect to their mutual origin by angle , as shown in Figure 1.a.

|  |  |
| --- | --- |
|  |  |
| 1. two dimensional coordinates | b)three dimensional coordinates |

From this geometrical setup it can be demonstrated that vector  can be uniquely defined in both frames as follows:

Figure 1. The same plane rotation considered with respect to two and three axes



Introducing the matrix notation for the linear transformation above results in a simple form that relates the vector  components in  frame to the corresponding components in frame:



The resulting rotation matrix is called a directional cosine matrix (DCM). The DCM matrix consists of the cosine and sine functions which are the direction cosines between corresponding axes of the new and old coordinate systems denoted in the superscript and the subscript correspondingly. Following the same approach, it can be demonstrated that for the case of right-handed coordinate system represented by three orthogonal axes (see Figure 1.b), the same right hand rotation results in transformation

,

where, for clarity, the subscript  denotes the axes of rotation. Proceeding similarly, right handed rotations of the coordinate frame about the  and axis give



It is worth noting that the DCM transformation has the following easy-to-remember properties that simplify its application, see more details in (Rogers 2003):

1. The transformed vector components along the axis of rotation remain unchanged with the rotation about that axis; elements of DCM are either 0 or1.
2. The remaining elements of DCM are either or functions of the angle of rotation.
3. The  elements are on the main diagonal with elements on off-diagonal.
4. The negative  component corresponds to the component rotated “outside” of the quadrant formed by the original frames.
5. Columns (rows) of a DCM matrix form an orthonormal set.

It is straightforward to verify that a DCM matrix have the following properties:



and therefore it belongs to a general class of orthonormal transformation matrices. For a sequence of rotations performed with respect to each orthogonal axis, the resulting transformation can be obtained by a matrix composed of three sequential rotations, called Euler angle rotations, starting from the original frame of reference, see Figure 2.



Figure 2. Three consecutive rotations.

Formally, this transformation is accomplished by rotating through the ordered sequence of Euler angles, where the numerical indexes define the ordered sequence of rotations.



It t is worth mentioning that the corresponding Euler angles are also widely used in notations, so that in the following formalism is possible. Therefore, a vector  described in one coordinate frame can be described in another coordinate frame of arbitrary orientation with respect to the original frame by a transformation matrix  composed of three sequential rotations as follows:





This matrix, that represents a transformation resulting from three sequential Euler angles rotations, will be used throughout the chapter.

Overall, any DCM matrix has a number of properties. They are summarized here for completeness; an interested reader is referred to reference (Goldstein 1980) for more details:

* Rotation matrices are orthogonal.
* The determinant of a rotation matrix is unity.
* Successive rotations can be represented by the ordered product of the individual rotation matrices.
* Rotation matrices are not commutative, hence, in general case.
* A nontrivial rotation matrix has only one eigenvalue equal to unity with other two, being a complex conjugate pair with unity magnitude; a trivial rotation is described by an identity matrix.

The time rate of change of the DCM matrix that defines the dynamics of the attitude states is important in derivation of the kinematic equations of motion. As it will be shown shortly, it enables relating the sensor measurements obtained in a body fixed frame to the time derivatives of the Euler angles describing the attitude of a body in an inertial frame.

Deriving the time derivative of a DCM matrix can be obtained by utilizing a linearization technique. Consider the variation of the DCM matrix resulting from three infinitely small consecutive rotations performed over an interval of time. Utilizing the small angle approximation of  and  and neglecting the higher order terms, it follows that:



Utilizing at any given time, the values of at the time can be expressed by

,

where . The time rate of change of the DCM matrix is then defined as



,

where



and is the vector of angular velocities. The rotation matrix  can be viewed as a rotation of the frame with respect to frame  measured in the frame. It can be observed that matrix is a skew symmetric matrix  and therefore the transposed equivalent of the rate of rotation is

.

Another useful general property of angular velocities is called the angular velocities addition theorem (Rogers 2003). The theorem states that for angular velocity vectors coordinated in a common frame, the resulting angular velocity of the cumulative rotation is a plain sum of the contributing rotations. Applying the theorem to  in results in, where  are the directional unity vectors defining the intermediate coordinate frames. Now, if a rotating frame is given by a set of time varying Euler angles  defined with respect to a stationary frame, then it is straightforward to determine the components of the angular velocity vector as though measured in the rotating frame. Starting from an initial stationary frame  (see Figure 2) and using two intermediate frames whose relative angular velocities are defined by the Euler angle rates, and utilizing the angular velocities addition theorem, the following kinematic equation can be obtained:

.

Substituting the corresponding DCM matrices from results in

.

Inverting the last equation results in equation



that defines the derivatives of the Euler angles in terms of the angles themselves and the rates as they were measured in the frame . These equations define the rotational kinematics of a rigid body; they contribute to the final set of 6DOF equations of motion.

Analysis of the equation shows that four elements of the inverted matrix become singular when the second rotation angle  approaches. This problem is usually called a *kinematic singularity* or a *gimbal lock* in navigation, and is one of the issues associated with the use of Euler angles for the attitude determination. For differently ordered Euler rotation sequences the kinematic singularity will occur at a different point. Therefore, one way to avoid the singularity is to switch or change the Euler angle sequences when approaching the singularity. Next, depending on the available computing power, the integration of the kinematic equation can be computationally expensive because it involves calculation of trigonometric functions. Furthermore, it can be observed that the Euler angles based DCM matrix is redundant; it requires only 3 out of 9 elements of the DCM matrix to uniquely define the Euler angles. These shortcomings usually result in applying different parameters describing the attitude and its dynamic transformation.

In applications to the fixed wing UAV attitude determination, the Rodriguez–Hamilton parameters, or quaternion, is one of the most widely used alternatives (Goldstein 1980). Utilizing the quaternion approach is very powerful because it gives a singularity-free attitude determination at any orientation of a rigid body. Next, since it can be shown that the equations of motion of a rigid body are linear differential equations in the components of quaternion, then it (linearity) is a desirable property, especially when developing estimation and control algorithms. Furthermore, the quaternion is a relatively computationally efficient approach since it does not involve trigonometric functions to compute the attitude matrix, and has only one redundant parameter, as opposed to the six redundant elements of the attitude matrix. However, it is also worth noting that the quaternion and Euler angles techniques are well connected with simple analytical representations of the DCM matrix and Euler angles through the parameters of quaternion. An interested reader is referred to an extensive historical survey of attitude representations (Shuster 1993) and references (Rogers 2003, Goldstein 1980) for more details in the alternative methods of attitude determination.

### Coordinate frames

Deriving equations of motion of a fixed wing UAV requires a definition of coordinate frames where forces and moments acting on the airplane can be conveniently defined and where the motion states including the position, velocity, acceleration and attitude can be suitably described. Considering the desired nomenclature of coordinate frames it is also important to account for a maximum duration of UAV mission and the corresponding operational range. With the latest advances in power technologies a long duration mission becomes a reality. As an example, the solar power technology is one of the alternatives that can make 24/7 flight of a fixed wing solar powered autonomous soaring gliders feasible. Thus, long duration and great operational distances require considering the UAV flight operations with respect to the rotating Earth. Therefore, in this subsection we define the following coordinate frames:

* 1. Earth-Centered-Earth-Fixed Frame {*e*}
  2. Geodetic Coordinate System {*λ, φ, h*}
  3. Tangent Plane Coordinate System {*u*}
  4. Body-Carried Frame {*n*}
  5. Body-Fixed Frame {*b*}
  6. Wind frame {*w*}

#### Depending on the duration of flight and operational range, both dictated by a specific UAV application, first three frames can be considered as inertial frames with the remaining three frames being body fixed. The inertial and body frames are related by a plain translation, while the body frames relate to each other by pure rotations. Details of the frames definition and their relations are the subject of this section.

#### Earth-Centered Earth Fixed and Geodetic Coordinate Frames

The *Earth Centered Earth Fixed* (ECEF) orthogonal coordinate system is fixed to the Earth and therefore it rotates at the Earth sidereal rate. The frame is usually marked with in subscript. It has its origin at the center of the Earth with  and axes placed in the equatorial plane and axis aligned with the direction of the Earth’s rotation vector, see Figure 3. The axis is usually attached to the intersection of the Greenwich meridian and the equator, and the axis completes the right hand system. It is worth noting, that the ECEF axes definition may vary, however the definition always states the attachment of two vectors to the direction of the earth rotation and the Greenwich meridian as the inherent Earth properties. The sidereal rate  is the rate of Earth rotation with respect to the distant stars (the true inertial frame). If necessary, for the purpose of UAV flight description this rate can be accurately approximated by one full rotation in 23h56’4.099” thus resulting in 15.04106718 deg/h.



Figure 3. ECEF and geodetic coordinate frames.

*Local Geodetic* { } frame is usually associated with the ECEF frame, see Figure 3. It has the same origin at the center of the Earth. The frame defines the orientation of the line normal to the Earth surface and passing through the point of interest. The orientation of the line is defined by two angles – geographic latitude and – geographic longitude, with the height above the Earth surface; these three parameters along with the components of velocity vector are the major navigation states. For the most UAV applications it is sufficiently accurate to model the Earth surface as an oblate spheroid with given -equatorial and -polar radiuses or one of the radiuses and the -ellipticity. Last revisited in 2004 datum of World Geodetic System (WGS-84) provides the following parameters for the oblate spheroid modeling: ,. The resulting transformation from the geodetic { } to the ECEF frame is as follows:



where - the eccentricity of oblate ellipsoid is defined as



#### Local Tangent Plane Coordinate System

The origin of the *Local Tangent Plane* (LTP) is fixed to the surface of the Earth with two of its axes attached to the plane tangent to the surface, see Figure 4. The frame is usually marked with the subscript and serves the purpose of an inertial frame in most of UAV applications. The frame’s  and axes are in the tangent plane and most often aligned with the North and East directions correspondingly, the  axis completes the right hand coordinate system, thus pointing down. Quite often the order and alignment of the LTP frame principal axes change. In such cases the LTP coordinate system explicitly specifies its type; in the nominal case presented above it can be also defined as an NED frame.

When the origin of LTP frame is defined in terms of its geographic latitude, longitude and altitude above the ground surface, then the equations can be applied to define the kinematics of navigation states.



Figure 4. Definition of the Local Tangent Plane; NED.

#### Body- Carried and Fixed Frames

In flight dynamics the body-attached reference frames usually have their origin at the center of gravity (CG) of an airplane, therefore these frames are moving. The *body-carried* frame  is an orthogonal frame originated at the CG of the UAV. All its axes are permanently stabilized and aligned with the LTP frame axes as it was connected to the CG, see Figure 5. This frame is connected to the LTP frame by means of a plain translation.



Figure 5. Definition of the body fixed frame with respect to LTP frame.

The *body-fixed* frame is an orthogonal frame defined with respect to the body-carried frame. Its origin is at the CG of UAV and its axes are rigidly connected to the body, therefore the frame rotates with the body. The frame is usually marked with the subscript. It can be proven (Goldstein 1980) that for every rigid body there is always an orthogonal coordinate system, usually called principal, in which the cross-products of inertia terms are zero. This feature is typical to bodies with planes of symmetry. Assuming, that a typical UAV has at least one plane of symmetry (geometric and mass symmetry), results in two of the body-fixed axes lying in the plane of symmetry. When the axes are aligned along the principal axes of inertia of the body, as it will be shown in the following chapter, the dynamic equations of motion become significantly simpler. In majority of fixed wing UAV configurations the axes of frame match the principal axes of inertia. The typical orientation of the body fixed axes is as follows (see Figure 5): if the UAV has a vertical plane of symmetry then  and lie in that plane of symmetry;  is points towards the direction of flight and  points downward and points right thus completing the right hand system.

As body moves, its attitude is defined with reference to the body-carried frame  by three consecutive Euler rotations by -yaw, -pitch and -roll angles. See their graphical illustration in Figure 2 where frames {0} and {1} relate to the frames and correspondingly. The formal definition of the Euler angles in the application to an airplane attitude specification is presented here for completeness:

* - yaw is the angle betweenand the projection of on the local horizontal plane.
* -pitch is the angle between the local horizon and the axis measured in the vertical plane of symmetry of UAV.
* -roll is the angle between the body fixed axis and the local horizon measured in the plane 

As it follows from the attitude representation section, the DCM matrix transforming the body-carried to the body-fixed  frame can be constructed as follows:



Here subscripts () denote the rotation from the LTP to the body fixed frame; and frames are always aligned by the definition of body-carried frame.

The application of the rotation matrix immediately follows from the need to describe the UAV translational motion in an inertial frame of reference by utilizing the inertial velocity measurements taken in the body fixed frame -. To this end, consider Figure 5 where vector denotes position of an airplane CG with respect to the LTP (NED) frame attached to the Earth. Relating the translational velocity and position, and accounting for the fact that *body-carried* frame is stabilized with respect to the non-rotating frame results



The relation between the Euler angles defining the relation between the stabilized frame and the body fixed frame  were already derived in -. They define the dynamics of Euler angles defined in an inertial frame with respect to the rates measured in the body fixed frame. Thus, the kinematic equations and represent the dynamics of translational and rotational coordinates, and therefore are the part of the final set of equations of motion.

#### Wind Frame

Aerodynamic forces and moments resulting from the body-air interaction as the airframe moves through the air depend on the body orientation with respect to the surrounding air. In other words, they depend on the vector representing the wind. The velocity vector calculated with respect to the possibly moving surrounding air (wind) is denoted, see Figure 6. The magnitude of  is called an *airspeed*; as opposed to the velocity vector defined in LTP with respect to the ground – *ground speed* vector. The orientation of the wind frame defined bywith respect to the body fixed is defined by two angles.



Figure 6. Wind frame and Body fixed frames. Definition of the angle of attack and the side slip.

To generate the lift force in flight, the wing of the UAV must be oriented at a positive angle with respect to the vector. This angle is called the *angle of attack*. The angle of attack is also one of the key parameters that define the longitudinal stability of an airplane. Therefore, quite often, the coordinate frame that results from a single rotation from the body-fixed frame on angle is called a stability frame (Beard and McLain 2012, Etkin and Reid 1995). As illustrated in Figure 6, the angle of attack is defined by the projection of into a vertical plane of symmetry of UAV (spanned by axes  in frame) and the longitudinal axis of UAV. It is positive when a leading edge of the wing rotates upward with respect to the. In turn, the angle between the velocity vector  projected into the “wing level” plane (spanned by axes  in frame) and the longitudinal axis of UAV is called the *side-slip angle*. It is denoted by.

Applying the DCM matrix approach to represent the complete transformation from the body fixed frameto the wind frameresults in the following:



The inverse transformation from the wind frame to the body fixed frame is the transpose of:.

The importance of the wind frame in application to UAVs flying in wind conditions that might contribute up to 100% of the nominal airplane speed cannot be overestimated. As an example, imagine an autonomous glider that is designed to utilize the wind energy to sustain the long duration flight. Therefore, it is necessary to clearly understand the difference between airspeed, represented by the velocity vector defined with respect to the air and the ground speed, represented with respect to the LTP frame. Consider the graphical representation of the relation between these vectors in Figure 7. In the presence of constant wind these velocities are related by the equation that is often called “wind triangle”:



where is the wind velocity defined in the LTP frame.




Figure 7. Wind triangle in 2D plane. Definition of the yaw, side slip and course over the angles.

The objective of the following development is to define the relations among these velocities defined in three different frames, while being measured or estimated by the algorithms and sensors installed in the body fixed and in the LTP frames. First, define the components of all three vectors in body fixed frame. Let the UAV velocity in LTP frame expressed in body frame be, and let the wind velocity in LTP frame expressed in body frame be. Observe, that  defined in frame can be expressed asand let be its components expressed in the body frame. Utilizing the definition of the angles of attack and sideslip relating the wind frame to the body-fixed frame and the “wind triangle” equation expressed in the body frame results in the following



This last equation relates the airspeed components of resolved in the body frame with the airspeed and the angles of attack and sideslip. In turn, if the wind components resolved in the body frame are known, then inverting the last equation allows for calculation of the airspeed and the  angles.



#### Generalized Motion.

In the development of dynamic equations of motion it will be necessary to calculate the absolute time derivative of a vector defined in coordinate frames that rotate and move with respect to each other. In an application to the UAV kinematics this can be justified by a necessity to relate the absolute time derivative of a position vector in inertial space (inertial velocity) that is defined based on the measurements taken in a body frame. Similarly, the second time derivative defines the body inertial acceleration.

Consider two coordinate frames {} and {}, where - stands for an inertial not rotating frame, and -stands for the rotating frame. The first objective is to calculate the derivative of a unity vector defined in {} attached to a rigid body rotating with respect to the {} with angular speed, see Figure 8. Denote the DCM transformation from {} to {} as.



Taking the derivative results in



where the time derivative of  is zero due to the rigid body assumption.



Figure 8. Deriving the time derivative of a vector.

Next, using the same setup, calculate the absolute time derivative of an arbitrary time varying vector defined in {}. Defining the vector in terms of its components in both frames and taking its time derivative in the inertial frame results

.

Taking the absolute time derivative of both expressions gives



Applying the previously obtained result allows to rewrite the last equation as



which expresses the derivative of the vector in inertial frame{} in terms of its change () calculated in a rotating frame {} and its relative rotation defined by the angular speed. The result in formally represents the Coriolis theorem. The second derivative of  defines a generalized expression for the body acceleration and is used in the development of the dynamic equations. The second derivative is obtained in a similar manner by recursively applying the Coriolis theorem, thus leading to





The following chapter heavily relies on the results in and when it develops the dynamic equations of motion.

#### Summary of Kinematics

This section developed the fundamental kinematic equations that not only define the kinematics of states and contribute to the final set of 6DOF equations of motion, but also serve as the basis for the design of the guidance and navigation tasks. There are numerous publications describing kinematics of moving frames. Most of the publications originate in the area of classical mechanics and rigid body dynamics. The publications in the area of flight dynamics and control always contain material addressing the attitude representation techniques and differential rotations and thus can be a good source of reference information. The most recent and thorough presentation of these topics can be found in (Beard and McLain 2012) where authors specifically address the kinematics and dynamics of small UAVs.

## Rigid Body Dynamics

This section addresses the development of the dynamics of a rigid body. The discussion is based on the application of the Newton’s laws for the cases of linear and angular motion. In particular, the second law of motion states, that the sum of all external forces acting on a body in an inertial frame must be equal to the time rate of change of its linear momentum. On the other hand, the sum of the external moments acting on a body must be equal to the time rate of change of its angular momentum. Applying these laws is the objective of this chapter.

We consider a fixed wing UAV as the rigid body and define its dynamics with respect to the body fixed coordinate system. Relations necessary to translate the inertial forces to the body fixed frame are also presented. Before proceeding to the derivation it is necessary to present some assumptions typical for the fixed wing UAVs:

* The mass of the UAV remains constant during the flight.
* The UAV is a rigid body.
* An Earth fixed frame can be considered as an inertial frame.

The relations derived in this chapter are general and can be applied to any rigid body; however, the treatment of the aerodynamic forces and moments acting on the body will be specific to the aerodynamically controlled fixed wing UAVs.

### Conservation of Linear momentum

First, assume that a rigid body consists of a set of -“isolated” elementary particles with mass  exposed to the external force while being connected together by the internal forces. Since the set of particles comprises a rigid body structure, the net force exerted by all the particles is . The set of external forces acting on the body is a combination of the gravity force acting in an inertial frame and the aerodynamic and propulsion forces defined with respect to the body fixed frame but expressed in inertial frame. Thus, the linear momentum of a single particle expressed in an inertial frame obeys the equality



It is worth noting that the time derivative is taken in an inertial frame as well, thus calling for the results in and . Summing up all  particles comprising the body gives the linear momentum equation of the entire body



The left part of this equation represents the sum of all forces (gravitational, propulsion and aerodynamic) expressed in an inertial frame, with the right part depending on the velocity of the body defined in an inertial frame. Observing that (i) the individual inertial velocities are not independent (they comprise a rigid body), assuming (ii) that the mass is constant, and utilizing the result in for the total velocity of the -th particle in an inertial frame, allows calculating the absolute time derivatives in an inertial frame in the following form



Here represents the angular velocity of the UAV body defined with respect to the inertial frame, see. Defining -the vector of CG location as, where  is the total mass of the body, simplifies the linear momentum equation.



Assuming that the location of CG does not change with time and applying the result in to the absolute derivatives of vectors and  results



where

- the externally applied forces expressed in the body frame;

- the inertial velocity components defined in the body frame;

- the body angular rates defined in the body frame;

- the body referenced location of the center of gravity;

Translation of the inertial forces to the body frame is justified by the convenience of calculating the local body frame derivatives of theandexpressed in the body frame; the first one results in , while the derivative of  is independent on the coordinate frame ().

Utilizing the double vector product identity  allows expanding the linear momentum equation in the most general scalar form as follows:



The last set of equations allows for the most general mass distribution inside the body. This set of equations might be useful when there is a need to model the placement of the body frame origin away from its CG. If the origin of the body-fixed frame is chosen at the CG, the last set of equations can be significantly simplified by substituting thus leading to



Expanding the cross product, results in the following form of the linear momentum equation.



Resolving equations with respect to the derivatives (accelerations in the body frame) leads to the standard form of differential equations suitable for immediate mathematical modeling.



### Conservation of Angular momentum

Applying the law of conservation of angular momentum to an -th particle in a moving frame is very similar to the approach used above. Consider a particle subjected to the internal and external moments. Similarly to the linear momentum case, the sum of internal moments acting on the particle should be equal to zero (), while the external moments arise from the inertial gravity and the body attached forces such as aerodynamic and propulsion. Thus, the conservation of angular momentum calculated across the entire rigid body results in



Since the sum of internal moments cancel, then applying the Coriolis theorem leads to



The first term can be expanded by utilizing the definition of the CG. 

Utilizing the double vector product identity allows expanding the second term as follows



The equation is obtained by recognizing the moments of inertia, their symmetrical properties and combining them into a matrix form defines the inertia tensor that allows converting the entire double vector product into a very compact form.



The diagonal terms of are called the moments of inertia. The off-diagonal terms are called the products of inertia, they define the inertia cross coupling. The moments of inertia are directly proportional to the UAV’s tendency to resist angular acceleration about a specific axis of rotation. For a body with axes of symmetry the inertia tensor has zero off-diagonal terms that significantly simplify its form and the final equations of angular momentum.

The last term in utilizes twice the same double cross product expansion, thus leading to



Denoting the body components of the total moment acting on the UAV as and combining the results in - lead to the following complete angular momentum equations in expanded form



In case of a typical UAV with a vertical plane of symmetry spanned by body fixed axes  the two pairs of the off-diagonal terms of  matrix become zero, namely and . This significantly simplifies the above equations:



These equations represent the complete rotational dynamics of a typical fixed wing UAV with a longitudinal plane of symmetry.

### Complete set of 6DOF Equations of Motion

The final set of 6DOF equations of motion describing the kinematics and dynamics of a generic UAV with a longitudinal plane of symmetry modeled as a rigid body can be summarized as follows:









Analysis of the above differential equations shows, that these equations are nonlinear and coupled, i.e., each differential equation depends upon variables which are described by other differential equations. In general case their analytical solutions are not known and they can only be solved numerically. There are 12 states describing the free motion of a rigid body subject to external forces () and moments (). In the control system design these variables are called state variables because they completely define the state of a rigid body at any instance of time. The state variables are summarized in Table 1.

Table 1. State variables of the 6DOF equations of motion.

|  |  |
| --- | --- |
| State variable | Definition |
|  | Vector of inertial position of the UAV and its components |
|  | Vector of inertial velocity components defined in the body-fixed frame |
|  | Euler angles that define the attitude of body-fixed frame with respect to the inertial frame |
|  | The body angular rates defined in the body-fixed frame |

What remains in the description of 6DOF equations of motion is to define the forces and moments acting on the airplane. This will be the objective of the next section.

## Forces and Moments Acting on the Airplane

The objective of this section is to present a generalized approach to defining the external forces and moments acting on a fixed wing UAV as functions of its states. The primary forces and moments acting on an airplane are the gravitational, thrust of the propulsion system, aerodynamic, and disturbances due to the flight in unsteady atmosphere. The most challenging task here is in defining the aerodynamic forces and moments resulting from the air-body interaction. Although the aerodynamic description of airfoils defining a fixed wing is not a new subject, the varieties of shapes, aspect ratios and aerodynamic configurations of modern fixed wing UAVs does not allow thorough presentation of all configurations. As an example, possible aerodynamic configurations of aerodynamic surfaces include tandem, variable span wings, joined wings, twin boom, V-tail configuration, just to name a few. However, a generalization is possible. An interested reader is referred to the most relevant survey (Mueller and DeLaurier 2003) of aerodynamics of small UAV that describes the modeling approaches and their limitations.

### Gravitation

Assuming that the flight altitude is negligible comparing to the radius of the Earth, it is sufficient to consider the gravity’s magnitude constant. Then, the effect of the Earth gravitation can be naturally modeled in the body-carried frame by the force applied to the CG of the UAV; the gravitational force is proportional to the gravitational constant  and is called weight of the UAV.



Before substituting this force expression into the equations of motion it needs to be transformed into the body frame. The inertial to body rotation  enables this transformation.



Since the gravitational force acts through the CG of the airplane, the corresponding moment contribution is zero,.

### Propulsion

The configuration of propulsion system of modern fixed wing UAVs varies greatly. The existing architectures can be categorized by the number of engines, their type, and their installation arrangement in the airframe. A thorough review of the existing architectures along with some future projections and trends in the modern and future UAV systems can be found in (OSD 2001). However, what is common across all possible configurations is that the vector of thrust in all systems is set parallel to the existing axes of symmetry; the thrust vectoring is not a common feature of fixed wing UAVs.

The thrust is naturally represented in the body fixed reference system. The direction of thrust vector  is usually fixed and lies in the plane of symmetry or is parallel to it; however it may not be aligned with the longitudinal -axis. If the orientation of thrust vector  varies in its reference to the airframe then a separate coordinate system analogous to the wind axes should be defined, thus introducing the required rotation of the thrust vector to the body fixed coordinate system. It is common design requirement that the installation of multiple engines should not introduce any unbalanced moments, thus not inducing any loss of control efforts for the UAV stabilization. For the analysis of a nominal flight regime the thrust vector  is considered fixed with respect to the body fixed frame.

For the sake of simplicity, consider a typical fixed wing UAV architecture where the installation of one or multiple engines results in the cumulative thrust vector passing through the CG, and the only moment being the torque generated by the reactive force from the rotating propeller. Thus, the net force of thrust in  direction and the moment around axis can be considered proportional to the thrust control command. Moreover, thrust characteristics of most conventional engines are always functions of the air density and the airspeed. Thus, the contributing force and moment resulting from the propulsion system can be presented as follows:



A particular example of modeling the propulsion force for the case of micro UAV can be found in (Beard and McLain 2012).

### Unsteady atmosphere

Turbulent atmosphere enters the equations of motion by changing the vector  resolved with respect to the air. In the previous discussion of the wind frame it was assumed that wind defined in the LTP frame is constant, thus the velocities are related by the “wind triangle” equation:



The most common approach (McRuer, Ashkenas and Graham 1999) in wind modeling is to consider two components contributing to the wind. The first one defines the steady wind in the Earth fixed frame, and therefore it can be presented by the measurements in LTP frame. The second component  is stochastic, that represents the short period disturbances or gusts expressed in the body fixed frame. Since the equations of motion are written in the body fixed frame, the LTP to body rotation serves the purpose of this transformation.



From the components of the wind and the UAV velocity, both resolved in the body frame, it is therefore possible to find the body frame components of the air velocity as



These body frame components of the air velocity enable straightforward calculation of the airspeed and the angles of attack and sideslip as



Modeling of the stochastic and steady components of wind is primarily based on experimental observations expressed using linear filters. The most widely used techniques are represented by von Karman and Dryden wind turbulence models (Hoblit 2001). Both methods are well supported with their numerical implementations.

### Aerodynamics

Aerodynamic forces and moments depend on the interaction of an aircraft with the airflow, which may be also in motion relative to the Earth. However, for the purpose of representing the nominal aerodynamic effects, the large-scale motion of the atmosphere is not critical and therefore will be considered constant; in fact it will only affect the navigation of the UAV.

The small perturbation theory (Ashley and Landahl 1985) is one of the approaches used in describing the aerodynamic interaction of a given aerodynamic shape with airflow. The perturbation in aerodynamic forces and moments are functions of variations in state variables and control inputs. The control inputs here are the deflections of the control surfaces of an airplane that modify the airflow around the body, thus generating the desired aerodynamic effects. The nomenclature of the control surfaces and their control mechanization depends on the particular aerodynamic composition of the airplane. Nevertheless, the principles describing the effects of the control surface deflection on the generated forces and moments are the same. Consider the following control effectors of a classical aerodynamic configuration: the elevator, the aileron, and the rudder (see Figure 9). In this configuration the ailerons are used to control the roll angle, the elevator is used to control the pitch angle, the rudder controls the yaw angle.



Figure 9. Control surfaces of a classical aerodynamic configuration.

Their deflections are denoted as - for the aileron, - for the elevator, and - for the rudder. The positive deflection of a control surface is defined by applying the right-hand rule to the rotation axis of the surface. The positive direction of the aileron, elevator and rudder deflections is also depicted in the .

Deflection of the control surfaces results in modification of the pressure distribution around the body. For example, deflecting elevator primarily changes the pitching moment acting on the airplane. In turn, this results in changing the angle of attack of the wing that increases the lifting power of the airplane. The calculation of aerodynamic characteristics of one or more lifting surfaces with variable deflections of the control surfaces at various attitudes with respect to the airflow can be accomplished by utilizing well-developed linear panel methods (Hess 1990, Henne 1990) conveniently implemented in various software packages (Fearn 2008, Kroo 2012).

The key result presented by the panel methods captures the effect of pressure distribution in the form of parameterized forces and moments versus the angles of attack and side-slip, and airspeed; they play a role of states here. For example, considering the longitudinal plane, the effect of pressure action acting on a fixed wing can be modeled using a total force and pitching moment acting on the wing. It is common to project the total force to the wind axes thus resulting in the lift  and drag force components. Figure 10 demonstrates the approach to modeling of aerodynamic effects in the wind and body fixed frames with respect to the vector of free airstream.




Figure 10. Definition of lift, drag and pitching moment in the wind frame.

As shown in the figure, the lift and drag forces act in the wind frame and are applied at the aerodynamic center of the lifting surface that is located at the quarter-chord point (- is length of the mean aerodynamic chord). The pitching moment acts around the aerodynamic center. Then, the forces and moment are represented in a form connecting a number of surface specific parameters and the states in the following form

,

where  are the nondimensional aerodynamic coefficients (to be parameterized),  is the planform area of the wing surface, and are the mean aerodynamic chord and the wing span. The same approach is applied to each of the aerodynamic surfaces comprising the airplane.

It is common practice to consider the total aerodynamic forces and moments in projections to the longitudinal and lateral planes of the airplane. The benefit of this approach is in simplicity of representing the aerodynamic effects and in providing a natural ground for the nonlinear model decomposition at the next step of the control system design. Thus, the longitudinal forces and moments consist of lift, drag and pitching moment acting in the vertical plane of symmetry. The lateral side force and yawing moment are caused by the asymmetric airflow around the airplane; the asymmetry can be caused by the side wind or intentional deflection of the rudder. For the majority of fixed wing UAVs the key states that define the parameterization of the aerodynamic coefficient are the angle of attack, side slip, body rates, and the controls are the surface deflections. The most general functional form of the longitudinal and lateral aerodynamics can be presented as follows.

Table 2. Parameterization of longitudinal and lateral aerodynamics

|  |  |
| --- | --- |
| Longitudinal channel | Lateral channel |
|  |  |

Without delving deeper into the intricacies of aerodynamic parameterization, it is sufficient to demonstrate the final form of forces and moments defined in the wind coordinate frame:

* longitudinal plane



* lateral plane



The presented parameterization is a simple linear approximation of the aerodynamics given by the Taylor series expansion taken with respect to the given trim conditions. The coefficients - are the nondimensional partial derivatives of the corresponding forces and moment (denoted in the subscript) taken with respect to the corresponding state or control (denoted in the superscript). The coefficients with zero in the subscript denote the forces and moments calculated when all states, including the control surface deflection, are zero; for example  denotes the roll moment coefficient estimated at. The common naming convention suggests, that those derivatives taken with respect to states  are called the stability derivatives, and those with respect to controls are called the control derivatives. Static stability of an aircraft with respect to disturbances in some variable is directly reflected in the sign of a particular derivative. For example, the sign of should be negative to guarantee static stability in pitching motion, while the sign of  should be positive for the directional static stability.

Each of the presented coefficients is usually a function of states. The precision requirement of the linear parameterization greatly depends on the operational envelop of the UAV and its intended use; the higher the maneuverability of the UAV the more terms are necessary to accurately represent the aerodynamics. Each of the coefficients has very intuitive physical meaning and is usually studied separately. An interested reader is referred to (Beard and McLain 2012) for a detailed discussion of the aerodynamic coefficients of small and micro fixed wing UAVs.

One last step need to be performed before the aerodynamics- defined in the wind coordinates can be plugged into the equations of motion - defined in the body fixed frame. The transformation from the wind to the body frame serves this purpose.

Therefore, the total forces and moments acting on the fixed wing UAV can be presented as follows:





## Conclusions

The objective of this chapter was to provide a review of the theoretical material required to enable accurate mathematical modelling of the free and controlled motion of a generic fixed wing UAV. The key building blocks presented were the coordinate frames and their transformations, kinematics of rotation, dynamics of motion, and the definition of forces and moments acting on the airplane. Kinematics of spatial rotation is what connects three building blocks of the “Kinematics-Dynamics-Actions” triad. Besides the 6DOF equations of motion describing the kinematics and dynamics of a rigid body motion, the tools and methods developed in this chapter contribute significantly into the UAV flight dynamics, system identification, control, guidance and navigation.

## References

* Ashley, Holt, and Marten Landahl. *Aerodynamics of Wings and Bodies(Dover Books on Aeronautical Engineering).* Dover Publications, 1985.
* Beard, Randal, and Timothy McLain. *Small Unmanned Aircraft: Theory and Practice.* Princeton University Press, 2012.
* Etkin, Bernard, and Lloyd Duff Reid. *Dynamics of Flight: Stability and Control.* 3rd. Wiley, 1995.
* Fearn, R.L. "Airfoil Aerodynamics Using Panel Methods." *The Mathematica Journal* (Wolfram Research) 10, no. 4 (2008): 15.
* Goldstein, Herbert. *Classical Mechanics.* 2 nd. Addison-Wesley, 1980.
* Henne, P. *Applied Computational Aerodynamics (Progress in Astronautics and Aeronautics).* AIAA, 1990.
* Hess, J.L. "Panel Methods in Computational Fluid Dynamics." *Annual Review of Fluid Mechanics* 22 (January 1990): 255-274.
* Hoblit, F.,. *Gust Loads on Aircraft: Concepts and Applications.* AIAA Education Series, 2001.
* Kroo, Ilan. "LinAir 4. A Nonplanar, Multiple Lifting Surface Aerodynamics Program." *DesktopAeronautics.* April 10, 2012. http://www.desktop.aero/linair.php (accessed April 10, 2012).
* McRuer, D., I. Ashkenas, and D. Graham. *Aircraft Dynamics and Automatic Control.* Princeton University Press, 1999.
* Mueller, Thomas J., and James D. DeLaurier. "Aerodynamics of Small Vehicles." *Annual Review in Fluid Mechanics*, 2003: 89-111.
* OSD. *Unmanned Aerial Vehicles Roadmap 2000 – 2025.* Washington , DC: Office of the Secretary of Defence, 2001.
* Rogers, Robert M. *Applied Mathematics in Integrated navigation Systems.* 2nd. Reston, Virginia: AIAA, 2003.
* Shuster, Malcolm D. "A Survey of Attitude Representations." *The Journal of Astronautical Sciences* 41, no. 4 (1993): 439-517.